Handleiding installeren Raspberry Pi
Stap 1 
Ik ben naar https://www.raspberrypi.com/software/ om de respberry pi imager te installeren. Heb de applicatie geïnstalleerd en met opgestart.
Stap 2: De micro sd kaart klaar maken
Ik heb gekozen voor de respberry pi 4 want dat is degene waar het erop gaat. [image: ]
Daarna heb ik respberry pi os gekozen.[image: ]
Ik heb de opslag apparaat gekozen [image: ]
Darnaa kon ik de os customison naar de hostnaam wachtwoord en wifi netwerk 
En gebruiker.[image: ]
Daarna heb ik het naar de card geflashed. En heb het in de respberry pi gestopt en het werkte meteen!
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Raspberry Pi 5
Respberry Pi 5, 500/ 500+, and Compute Module 5

Raspberry Pi 3
Raspberry Pi 3 Model A+ / B/ B+ and Compute Module 3 /
3

Raspberry Pi 2
Respbery Pi 2 Model B

Raspberry Pi 1
Raspberry Pi 1 Model A/ A+ / B/ B+ and Compute Module 1
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Choose operating system

Select an operating system to install on your Raspberry Pi

Raspberry Pi 0S (32-bit)
A port of Debian Trixie with the Raspberry Pi Desktop
Online-1.2 GB cownlosd
Released: 20260915

Raspberry Pi OS (Legacy, 32-bit)
‘ A port of Debian Bookworm with securty updates and

desktop environment
Online-1.2 GB download

Released: 2026-09-15
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Opslagapparaat Write complete!
Customisation
Your choices:
Hostname Device: Raspberry Pi 4
Localisation Operating system:  Raspberry Pi OS (64-bit)
Uoar Storage: Mass Storage Device USB Device
W Customisations applied:
Remote / Hostname configured
S— 7 loesion g
7 Wi configured
Witing 7 55H enabled
7 Raspberry Pi Connect enabled
The sorage device was efected automatically. You can now remove
safely.

APP OPTIONS WRITE ANOTHER FINIS




